Detention Series
(Detention Fire Extinguisher, Hose and Fire Department Valve Cabinets)

BOX SPECIFICATION: All recessed and surface-mounted cabinets feature 12 gauge cold-rolled steel boxes finished with a rust inhibitive baked primer. Surface-mounted cabinets with stainless steel trim and door have a box constructed entirely of 304 stainless steel with industrial matte finish.

TRIM AND DOOR SPECIFICATION: Steel trims and doors are manufactured entirely from 12 gauge cold-rolled steel. The doors are one piece construction. Standard finish is a rust inhibitive backed primer. Stainless steel trims and doors feature the same construction using 12 gauge 304 stainless steel with industrial matte finish.