IE144T
(4" 300lb Rated Threaded Check Valve)

Wilson and Cousins Model IE144T 300lb Rated UL/ULCApproved Thread x Thread spring loaded Check Valve suitable for horizontal or vertical installation (upward flow only)