IE144TG
(4" 300lb Rated Threaded x Groove Check Valve)

Wilson and Cousins, IE144TG, 300lb Rated UL/ULC Approved, Male Thread x Groove spring loaded Check Valve suitable for horizontal or vertical installation (upward flow only)