IE1BR-COMBO
(66"(1674) X 34"(864) X (2) 8"(203) Recessed style combination double hose cabinet)

Wilson & Cousins, IE1BR-COMBO, is a recessed 66"x34"x (2)8" (1674mm x 864mm x 203mm) type combination double section zone control valve and fire hose cabinet. The cabinet is constructed with one common frame and two doors of 16 gauge Cold Rolled Steel. Valve section to be full metal and fire hose section to be full glass opening. Frame to have 2" adjustment to wall. The fire tub to be 30"x30"x8" (762mm x 762mm x 203mm) and the valve tub to be 30"x30"x8" (762mm x 762mm x 203mm) and both comes with valve knockouts. The interior and exterior of the cabinet is treated for corrosion resistance by an electrostatically applied oven-baked primer finish. The doors and frames are fitted with a full length 180-degree opening semi-concealed piano hinges, stainless steel concealed latches and 3/16" (5mm) clear glass.