IE1BR-COMBO-SS
(66"(1674) X 34"(864) X (2) 8"(203) Recessed style combination double hose cabinet with SS door)

Wilson & Cousins, IE1BR-COMBO-SS, is a recessed 66" x 34" x (2)8" (1674mm x 864mm x 203mm), combination double section zone control valve and fire hose cabinet. The cabinet is constructed with one common frame and two doors of 14-gauge #4 satin stainless steel door and frame and 16-gauge Cold Rolled Steel prime painted tub. Valve section to be full metal and fire hose section to be full glass opening.  Frame to have 2" adjustment to wall. The fire tub to be 30"x30"x8" (762mm x 762mm x 203mm) and the valve tub to be 30"x30"x8" (762mm x 762mm x 203mm).  Both comes with valve knockouts.  The interior and exterior of the tubs are treated for corrosion resistance by an electrostatically applied oven-baked primer finish. The doors and frames are fitted with a full length 180-degree opening semi-concealed piano hinges and stainless-steel concealed latches.