IE23-HPCP
(2.5" Polish Chrome Standard Angle Hose Valve.  2.5" Female Inlet x 2.5" Male Hose Thread Outlet.)

Wilson & Cousins, IE23-HPCP, UL/ULC listed and FM Approved 300 lbs (2070 kPa) pressure tested cast brass with polish chrome finish, standard angle hose valve.  The valve will be used where standpipe pressure at the inlet of the valve is less than 100 psi (689 kPa).