IE23-PRV-CP
(2.5" Chrome Pressure Restricting Angle Valve with Female NPT Inlet x Male Hose Outlet.)

Wilson & Cousins, IE23-PRV-CP, UL/ULC listed and FM Approved 300 lbs (2070 kPa) pressure tested cast brass with chrome finish, pressure restricting angle hose valve where standpipe pressure at the inlet of the valve is less than 175 psi (1207 kPa) and greater than 100 psi (689 kPa).