IE23-PRVFF
(2.5" Pressure Restricting Angle Valve with Female NPT Inlet x Female NPT Outlet.)

Wilson & Cousins, Model IE23-PRVFF, UL/ULC listed and FM Approved, 300 lbs (2068 kPa) pressure tested, cast brass, pressure restricting angle hose valve where standpipe pressure at the inlet of the valve is less than 175 psi (1207 kPa) and greater than 100 psi (689 kPa).