IE25HM-PRV-CP
(1.5" Chrome Pressure Restricting Angle Valve with hydrolator Female NPT Inlet x Male Hose Outlet.)

Wilson & Cousins, IE25HM-PRV-CP, UL/ULC listed and FM Approved 300 lbs (2070 kPa) pressure tested cast brass with chrome standard finish pressure restricting angle hose valve where standpipe pressure at the inlet of the valve is less than 175 psi (1207 kPa) and greater than 90 psi (620 kPa).