IE2600-15-FF-SS
(1-1/2" Female x Female Factory Set Pressure Reducing Angle Valve with Supervisory Switch)

Wilson & Cousins, IE2600-15-FF-SS Series:

•	Pressure reducing angle (90-degree) valve
•	Cast brass construction
•	Integral supervisory switch for remote monitoring of open or closed position
•	Maximum inlet pressure up to 400 psi (2758 kPa)
•	Maximum inlet flow rate up to 250 GPM
•	Seven (7) different bonnet sizes to choose from-each one offering different reduction properties
•	UL/ULC Listed