IE2600-25-FM
(2-1/2" Female x Male Factory Set Pressure Reducing Angle Valve)

Wilson & Cousins, IE2600-25-FM Series:

•	Pressure reducing angle (90-degree) valve
•	UL/ULC Listed
•	Cast brass construction
•	Maximum inlet pressure up to 400 psi (2758 kPa)
•	Maximum inlet flow rate up to 500 GPM
•	Eight (8) different bonnet sizes to choose from-each one offering different reduction properties