IE28-4AT
(4.0" NPT x (2)2.5" NPT - Angled Recessed Brass FDC w. Double Drop Clappers)

Wilson & Cousins, IE28-4AT, 4" (100mm) F NPT x 2.5" (65mm) F NPT x 2.5" (65mm) F NPT, cast brass, angled (90-Degree), recessed (flush-mount) body fire department connection. Each 2.5" (65mm) inlet can supply up to 250 GPM. UL /ULC Listed and FM Approved.