IE33S PAC CP
(4"x2.5"X2.5" Chrome straight body exposed fire department connection with chrome accessories)

Wilson & Cousins, IE33S PAC CP, 4" (100mm) NPT x 2.5" (65mm) hose thread x 2.5" (65mm) hose thread cast brass, chrome finish, exposed straight body fire department connection with chrome accessories. Each 2.5" (65mm) inlet can supply up to 250 GPM and to suit type of threads on those used by local fire department.  UL /ULC Listed and FM Approved body. The fire department connection comes with two plugs and chains and signage having letters at least 1" (25mm) in size, cast on plate or cast on fitting.