IE39-A
(4-Way Square Siamese Connection - 6" NPT x (4)3" NPT)

Wilson & Cousins, IE39-A, square siamese features four (4) 3" NPT connections spaced at 7" (178mm) centers and perpendicular to a single (1) 6" NPT. A 2" NPT threaded drainage point is provided on the top of the unit, opposite of the 6" connection.

The entire manifold is composed of cast brass and is rated for operating pressures up to 175 psi (1206 kPa) and able to supply a minimum capacity of 1000 G.P.M.  UL Listed.