IE2600A-S-25-FF
(2-1/2" Female x Female Field Adjustable Pressure Reducing Inline Valve)

Wilson & Cousins, IE2600A-S-25-FF Series:

•	Field adjustable, pressure reducing inline (straight) valve
•	Forged brass construction
•	Maximum inlet pressure up to 400 psi (2758 kPa)
•	Maximum inlet flow rate up to 500 GPM
•	Seven (7) different spring settings to choose from-each one offering different reduction properties
•	UL/ULC listed
•	The valve is used when the pressure at the inlet of the valve is greater than 175 psi (1207 kPa), based on NFPA 13