IE25H-CP 
(1.5" Chrome Angle Valve with hydrolator Female NPT Inlet x Female NPT Outlet.)

Wilson & Cousins, Model IE25H-CP, UL/ULC listed and FM Approved, 300 lbs (2068 kPa) pressure tested cast brass, chrome finish, standard angle hose valve.  The valve will be used where standpipe pressure at the inlet of the valve is less than 90 psi (620 kPa).