IE2600A-A-15-FM
(1-1/2" Female x Male Field Adjustable Pressure Reducing Angle Valve)

Wilson & Cousins, IE2600A-A-15-FM Series:

•	Field adjustable, pressure reducing angle (90-degree) valve
•	Cast brass construction
•	Maximum inlet pressure up to 340 psi (2344 kPa)
•	Maximum inlet flow rate up to 250 GPM
•	Six (6) different spring settings to choose from-each one offering different reduction properties
•	UL/ULC listed
•	The valve is used when the pressure at the inlet of the valve is greater than 175 psi (1207 kPa), based on NFPA 14