HF325F
(Female Cast Brass Check Snoot (Clapper Style) - 3" FNPT x 2-1/2" Hose Swivel)

Wilson & Cousins, HF325F, 3" (76mm) F NPT x 2.5" (65mm) F swivel hose thread, polished brass Check Snoot. The 2.5" (65mm) inlet can supply up to 250 GPM. UL /ULC Listed and FM Approved.