Hose 2 1/2" 50SJ
(2.5” x 50ft Single Jacket Hose)

Wilson and Cousins, HOSE 2 ½” 50SJ, 2-1/2" (64mm) x 50’ (15.25m) Single Jacket Industrial hose synthetic rubber lined, mildew and rot resistant. Comes with Aluminum Couplings.  Meets or exceeds requirements for NFPA 1961, UL and FM.