IE141 CP LEXAN
(IE141 Chrome Swing Rack - 1.5" x 100' Rack Hose w/ Chromed Couplings and Lexan Nozzle)

Wilson & Cousins, IE141 CP LEXAN, chrome swing rack package that comes with the following:

•Semi-automatic chrome swing rack MODEL IE141 with water stop, UL/ULC Listed and FM Approved
•100’ (30.5m) Single Jacket Rack Hose, UL/ULC Listed
•Chrome plated forged brass couplings
•1.5” (38mm) chrome plated, lexan, adjustable straight-stream fog nozzle