IE2600-25-SG
(2-1/2" Groove x Groove Factory Set Pressure Reducing Inline Valve)

Wilson & Cousins, IE2600-25-SG Series:

•	Pressure reducing inline (straight) valve
•	UL/ULC Listed
•	Cast brass construction
•	Maximum inlet pressure up to 400 psi (2758 kPa)
•	Maximum inlet flow rate up to 500 GPM
•	Eight (8) different bonnet sizes to choose from-each one offering different reduction properties