IE284C PACK
(4"x2.5"x2.5" Recessed straight body fire department connection chrome package)

Wilson & Cousins, IE284C PACK, 4" (100mm) grooved x 2.5" (65mm) NPT x 2.5" (65mm) NPT, cast brass recessed straight body fire department connection with brass, chrome finish accessories. Each 2.5" (65mm) inlet can supply up to 250 GPM and to suit type of threads on hose used by local fire department, the body is UL /ULC Listed and FM Approved.  The fire department connection comes with two snoots and swivels, plugs with chains and signage having letters at least 1" (25mm) in size, cast on plate.