IE33S HPCP
(4"x2.5"X2.5" Polish chrome straight body exposed fire department connection)

Wilson & Cousins, IE33S HPCP, 4" (100mm) NPT x 2.5" (65mm) hose thread x 2.5" (65mm) hose thread cast brass, chrome finish, high polish exposed straight body fire department connection. Each 2.5" (65mm) inlet can supply up to 250 GPM. UL /ULC Listed and FM Approved.