IE34S PAC RED
(4"x2.5"X2.5" Brass angle body exposed fire department connection with red accessories)

Wilson & Cousins, IE34S PAC RED, 4" (100mm) NPT x 2.5" (65mm) hose thread x 2.5" (65mm) hose thread cast brass, exposed angle body fire department connection with red accessories. Each 2.5" (65mm) inlet can supply up to 250 GPM and to suit type of threads on those used by local fire department. UL /ULC Listed and FM Approved. The fire department connection comes with two red quick plugs and signage having letters at least 1" (25mm) in size, cast on plate or cast on fitting.