IE75 CP LEXAN
(IE75 Chrome Swing Rack - 1.5" x 75' Rack Hose w/ Chromed Couplings and Lexan Nozzle)

Wilson & Cousins, IE75 CP LEXAN, chrome swing rack package that comes with the following:

•Semi-automatic chrome swing rack MODEL IE141 with water stop, UL/ULC Listed and FM Approved
•75’ (23m) Single Jacket Rack Hose, UL/ULC Listed
•Chrome plated forged brass couplings
•1.5” (38mm) chrome plated, lexan, adjustable straight-stream fog nozzle