IE75 RED LEXAN
(IE75 Red Swing Rack - 1.5" x 75' Rack Hose w/ Brass Couplings and Lexan Nozzle)

Wilson & Cousins, IE75 RED LEXAN, red swing rack package that comes with the following:

•Semi-automatic red swing rack MODEL IE141 with water stop, UL/ULC Listed and FM Approved
•75’ (23m) Single Jacket Rack Hose, UL/ULC Listed
•Forged brass couplings
•1.5” (38mm) red lexan, adjustable straight-stream fog nozzle, FM Approved