IE29-63T
(6.0" NPT x (3)3.0" NPT – Inline Exposed Brass Roof Manifold)

Wilson & Cousins, IE29-63T, 6" (152mm) F NPT x (3) 3" (76mm) F NPT, cast brass, inline building connection.  An exposed body, fire department connection. Each 3" (76mm) inlet can supply up to 250 GPM.  UL Listed.