IE30
(Wall Type Chrome Hydrant Control Valve with Square Plate)

Wilson & Cousins, IE30, cast brass, chrome plated, Wall Hydrant Control Valve package to attach to 4” NRS Gate Valve (supplied by others) with an 18” steel extension rod and brass coupling.  The Control Valve coincides with a recessed (flushed) Wall Hydrant.