IE34D-630
(6.0" NPT x (2)3.0" Hose Swivel - Angle Exposed Brass FDC w. Double Drop Clappers)

Wilson & Cousins, IE34D-630, 6" (152mm) NPT x 3" (76mm) hose thread x 3" (76mm) hose thread, cast brass exposed angle body fire department connection with double clappers. Each 3" (76mm) inlet can supply up to 250 GPM. Rated working pressure of 175 psi.  UL /ULC Listed and FM Approved.