HF325M CP
(Male Chrome Check Snoot (Clapper Style) - 3" MNPT x 2-1/2" Hose Swivel)

Wilson & Cousins, HF325M CP, 3" (76mm) M NPT x 2.5" (65mm) F swivel hose thread, polished chrome Check Snoot. The 2.5" (65mm) inlet can supply up to 250 GPM. UL /ULC Listed and FM Approved.