IE33P-CP 6.0
(Chromed Cast Brass Round Plate for Exposed F.D.C. with 6" NPS Hole)

Wilson & Cousins, IE33P-CP 6.0, brass, chrome plated circular escutcheon plate is used to identify and trim exposed fire department connections, such as the IE33D and IE34D series of connections. Identification of connection type is designated with cast letters appearing at least 1" (25mm) in size.

Use with connections having one (1) 6" NPS (DN 152) outlet.