IE37-63T
(6.0" NPT x (3) 3.0" NPT – Inline Exposed End Inlet Brass Roof Manifold)

Wilson & Cousins, IE37-63T, 6" (152mm) F NPT x (3) 3" (76mm) F NPT, cast brass, inline end inlet building connection.  An exposed body, fire department connection. Each 3" (76mm) inlet can supply up to 250 GPM.  The connection has a rated operating pressure up to 300 psi.  UL Listed.